;/*++
;
;Copyright (c) 2013 Intel Corporation
;
;Module Name:
;    iaiouart.inf
;
;Abstract:
;    INF file for installing UART Controller driver
;
;Installation Notes: 
;    Using Devcon: Type "devcon update iaiouart.inf ACPI\INT33C4" to install on FPGA platforms
;    Using Devcon: Type "devcon update iaiouart.inf ACPI\INT33C5" to install on FPGA platforms
;
;--*/

[Version]
Signature="$WINDOWS NT$"
Class=System
ClassGuid={4D36E97D-E325-11CE-BFC1-08002BE10318}
Provider=%INTEL%
DriverVer=11/15/2013,603.9600.2801.29953

CatalogFile = iaiouart.cat

[DestinationDirs]
DefaultDestDir = 12

; ================= Class section =====================

;[ClassInstall32]
;Addreg=SampleClassReg     

;[SampleClassReg]
;HKR,,,0,%ClassName%
;HKR,,Icon,,-5

[SourceDisksNames]
1 = %DiskId1%,,,""

[SourceDisksFiles]
iaiouart.sys  = 1,,

;*****************************************
; iaiouart Install Section
;*****************************************

[ControlFlags]
ExcludeFromSelect=*

[Manufacturer]
%INTEL%=Intel,NTx86

; For XP and later
[Intel.NTx86]
; DisplayName               Section             DeviceId         CompatibleId
; -----------               -------             --------         ------------
%iaiouart.DeviceDescE6%= iaiouart_Inst,   ACPI\80860F0A,   ACPI\INT33BC

[iaiouart_Inst.NT]
CopyFiles=Drivers_Dir

[Drivers_Dir]
iaiouart.sys

;-------------- Service installation
[iaiouart_Inst.NT.Services]
AddService = iaiouart,%SPSVCINST_ASSOCSERVICE%, iaiouart_Service_Inst

; -------------- iaLPSS_UART driver install sections
[iaiouart_Service_Inst]
DisplayName    = %iaiouart.SVCDESC%
ServiceType    = 1               ; SERVICE_KERNEL_DRIVER
StartType      = 3               ; SERVICE_DEMAND_START 
ErrorControl   = 1               ; SERVICE_ERROR_NORMAL
ServiceBinary  = %12%\iaiouart.sys
LoadOrderGroup = Extended Base
Dependencies   = SerCx

[Strings]
SPSVCINST_ASSOCSERVICE= 0x00000002
INTEL = "Intel Corporation"
StdMfg = "(Standard system devices)"
DiskId1 = "UART Controller Installation Disk #1"
iaiouart.DeviceDescE6 = "UART Controller"
iaiouart.SVCDESC = "UART Controller"
