;/*++
;
;Copyright (c) 2009-2014 Intel Corporation All rights Reserved
;
;Module Name:
;
;    GYRO_SensorDriver.inf
;
;Abstract:
;    INF file for installing Gyroscope BMG160 driver
;
;Installation Notes:
;    Using Devcon: Type "pnputil -i -a GYRO_SensorDriver.inf" to install
;
;--*/

[Version]
Signature="$WINDOWS NT$"
Class=System
ClassGuid={4D36E97D-E325-11CE-BFC1-08002BE10318}
Provider=%ManufacturerName%
CatalogFile=GYRO_SensorDriver.cat
DriverVer=06/27/2014,9.59.48.710
PnPLockDown=1

[DestinationDirs]
DefaultDestDir = 12

[SourceDisksNames]
1 = %DiskName%,,,""

[SourceDisksFiles]
GYRO_SensorDriver.sys  = 1,,

;*****************************************
; Install Section
;*****************************************

[Manufacturer]
%ManufacturerName%=Intel,NTx86

[Intel.NTx86]
%GYRO_SensorDriver.DeviceDesc%=GYRO_SensorDriver_Device, ACPI\BSBG0160

[GYRO_SensorDriver_Device.NT]
CopyFiles=Drivers_Dir

[Drivers_Dir]
GYRO_SensorDriver.sys

;-------------- Service installation
[GYRO_SensorDriver_Device.NT.Services]
AddService = GYRO_SensorDriver,%SPSVCINST_ASSOCSERVICE%, GYRO_SensorDriver_Service_Inst

; -------------- GYRO_SensorDriver driver install sections
[GYRO_SensorDriver_Service_Inst]
DisplayName    = %GYRO_SensorDriver.SVCDESC%
ServiceType    = 1               ; SERVICE_KERNEL_DRIVER
StartType      = 3               ; SERVICE_DEMAND_START
ErrorControl   = 1               ; SERVICE_ERROR_NORMAL
ServiceBinary  = %12%\GYRO_SensorDriver.sys
Dependencies   = SpbCx
LoadOrderGroup = Extended Base

;
;--- GYRO_SensorDriver_Device Coinstaller installation ------
;

[GYRO_SensorDriver_Device.NT.HW]
AddReg=GYRO_SensorDriver_AddReg

[GYRO_SensorDriver_AddReg]
HKR,"Settings",internal,0x00000010,1

[Strings]
SPSVCINST_ASSOCSERVICE= 0x00000002
ManufacturerName="Intel Corporation"
DiskName = "BSBA0150 Installation Disk #1"
GYRO_SensorDriver.DeviceDesc = "Gyroscope Sensor Gyro"
GYRO_SensorDriver.SVCDESC = "BOSCH BMG160 GYRO Device Driver"
