 This driver is to solve the win10 no audio problem.
1. Bios version must be：
AD0J0162.bin
MD5:3FB2D774E8A35371AACA9C0AEE47ABF9
SHA1:9C4197B09F2E22C06F65F8806264586723380DE2
CRC32:E96E1A41

What is this Blos version for?

NE0 Z100-0dB does not natively support Windows 10 Os, because the status ofthe audio driver will not be correctly displayed.
This BlOS version is to resolve this problem.
So, in a word, it's recommended to install this BlOS version ONLY if you need
to install Windows 10 OS on the NEO Z100-0dB.

Instructions to install the this Blos:
a. Boot the device and enter the Windows OS.
b. Right-click the file 'FlashBlOS.bat' and choose 'Run as Administrator'.
c. Wait for a minute or two, until the installation is finished.


2. Install the driver package“Intel_SST_ADL_RPL_v10.29.00.9677.zip”